This thesis introduces a innovative way to connect small \gls{IoT} devices to
high level \gls{TOP} implementations languages. It demonstrates how a novel
frontend for the existing class-based shallowly \gls{EDSL} called \gls{mTask}
by Koopman et al.\ --- written in \gls{Clean} --- can be employed to compile
\gls{IoT}-\glspl{Task} on the fly and send them to devices as interpretable
bytecode. All of which adheres to the \gls{TOP} philosophy where common
concepts such as \glspl{SDS} and \gls{Task}-combinators are available at ease.
