This thesis introduces a way to connect small \gls{IoT} devices with high level
\gls{TOP} implementations languages. It demonstrates how a new frontend for the
class-based shallowly \gls{EDSL} called \gls{mTask} written in \gls{Clean} can
be employed to compile \gls{IoT}-tasks on the fly and send them to devices as
interpretable bytecode. All of which adheres to the \gls{TOP} philosophy where
common concepts such as \glspl{SDS} and task-combinators are available at ease.
