The existing \gls{C}-backend for the \gls{mTask}-\gls{EDSL} generates a
self-contained \gls{iTasks} like \gls{TOP} system for microcontrollers. The
added view for the \gls{mTask}-\gls{EDSL} does not result in a
self-contained system but compiles the expressions to bytecode representing a
single \gls{Task}. The device and the server communicate using the
Leader/Follower principle\footnote{Also known as Master/Slave}. Only the server
can initiate a connection with a device and only the server can produce and
send \glspl{Task} to the device. Concepts such as \glspl{SDS} are available on
the device and are the main use of communication between the client and the
server.

Chapter~\ref{chp:arch} elaborates on the considerations and implementation of
the system.
