The original \gls{C}-backend for the \gls{mTask}-\gls{EDSL} generated a
self-contained \gls{iTasks} like \gls{TOP} system for a microcontroller. The
proposed backend for the \gls{mTask}-\gls{EDSL} does not result in a
self-contained system but only compiles the expressions to bytecode. The device
and the server communicate using the Leader/Follower principle\footnote{Also
known as Master/Slave}. Only the server can initiate a connection with a device
and only the server can produce and send \glspl{Task} to the device. Concepts
such as \glspl{SDS} are available on the device and are the main use of
communication between the client and the server.

Chapter~\ref{chp:arch} elaborates on the considerations and implementation of
the system.
